Reccomendation:
Material - PLA
Support - No
Brim - No
Nozzle size - 0,4mm

Attention:
Depending on the use of the product, it is necessary to take into account the properties (specification) of the material used for printing.
- Ambient temperature of use. Usually PLA material becomes elastic at approximately 60 degrees. At 70 - the material is clearly soft, easily deformed.
- Flammability class. Usually PLA materials only meet the UL94 HB class, but there are special mixtures that reach UL94 V0